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Background:
This DS supersedes and replaces DS 2021/001 following its 5 year review

	Question: What are the requirements that an ExCB must comply with for the issue of Certificates of Conformity to IEC TS 60079-46:2017


	
ANSWER:  An ExCB shall:

1. Have ISO 80079-36 and ISO 80079-37 within their scope prior to being able to issue IECEx Certificates according to IEC TS 60079-46.

1. In accordance with IECEx 02 rules and OD 009, IECEx Certified Equipment Scheme, Procedures for the Issuing of IECEx Certificates of Conformity, IECEx Test Reports and IECEx Quality Assessment Reports ExCBs, ExCBs can only accept IECEx Certificate applications for assemblies where the ExCB has all Ex protection techniques, associated with the Equipment Assembly, within their scope.

1. Provide Certificate information and Marking requirements in accordance with IEC TS 60079-46:2017

1. List only the following standards on the Certificate of Conformity
3. IEC TS 60079-46:2017
3. IEC 60079-0 must always be identified (as it is required for both electrical and non-electrical evaluations).
3. ISO 80079-36:2016



Additionally:
Clause 6.4 of IEC TS 60079-46:2017 requires the Manufacturer to perform and document an assessment of all ignition hazards in accordance with ISO 80079-36 for both non-electrical and electrical risks. 
In this context the ExCB/ExTL shall confirm that such an ignition hazard assessment has been conducted and documented by the manufacturer.  The ExCB/ExTL shall review the ignition hazard assessment and shall be satisfied that it has been conducted in accordance with ISO 80079-36 and that the conclusions are appropriate. It is not expected that the ExCB/ExTL repeat the ignition hazard assessment conducted by the manufacturer; however  they shall have sufficient evidence that the assessment has been adequately performed and is acceptable. 
Where the ExCB/ExTL is not satisfied that the ignition hazard assessment has been conducted as required, then the ExCB/ExTL may request the manufacturer to conduct additional   work.  
The following text is to be added to the equipment description field of the certificate as confirmation that this has been completed and subsequently confirmed by the ExCB as satisfying the requirements for ignition hazard assessments.
‘It is confirmed that the ignition hazard assessment has been conducted to ISO 80079-36 by the Manufacturer,

NOTE: Mention of this confirmation shall also be included in the ExTR.
 


	This DS is applicable to:
 projects commenced prior to publication of the DS; AND
 all certifications issued after its publication; OR
 only for the new certifications (Issue No. 0) and their subsequent revisions.


NOTE: The following should be noted when developing ExTAG Decision Sheets:
The development process should be in compliance with IECEx OD 035.
The purpose for development of ExTAG Decision Sheets is to unify the application of the Standards used in the IECEx System and is not intended to modify or "interpret" Standards.
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